AGH150W-4

Coupling device to expand the nominal voltage range of the ISOMETER® IRDH275/375 on AC 0...1150 V, DC 0...1760 V. 

The sealable enclosure is suited for quick DIN rail mounting.

Manufacturer:
Bender GmbH & Co. KG
Londorfer Str. 65
35305 Gruenberg
Telephone: +49 6401/807-0 
Fax: +49 6401/807-259

Type: AGH150W-4